(footprint "0.91 oLED DSP"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 19 3.47 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "e37a0f54-c7d0-47b4-a5d2-bacb8401854f")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "0.91 oLED DSP"
		(at 19 8.63 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "71999331-f75f-4cc7-ab83-479da53c1dfb")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "fdab4f9e-8eef-40ed-a135-92ec03f61c03")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "1e51ab5a-df75-4661-8aa8-e59e3001dc91")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_rect
		(start 0 0)
		(end 38 12)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill no)
		(layer "F.SilkS")
		(uuid "ed5c046d-5ecd-44b9-865b-8bccfc643e91")
	)
	(fp_text user "${REFERENCE}"
		(at 19 6 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "350c0fbd-12d7-44d1-addc-bccd628c9a08")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole circle
		(at 1.5 9.81)
		(size 1.8 1.8)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "e757b9c8-013a-4e8e-aeff-f9232cf1ad65")
	)
	(pad "2" thru_hole circle
		(at 1.5 7.27)
		(size 1.8 1.8)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "ef36f0dc-1437-416f-b0ae-026993519d5f")
	)
	(pad "3" thru_hole circle
		(at 1.5 4.73)
		(size 1.8 1.8)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "e6242414-ddba-4813-aab5-e541972f8c68")
	)
	(pad "4" thru_hole circle
		(at 1.5 2.19)
		(size 1.8 1.8)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "4aecc1dc-c011-4062-bd0c-719af728b3e9")
	)
	(embedded_fonts no)
)
