(footprint "KF211V-5.0" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr through_hole)
  (fp_text reference "REF**" (at -4.3 -17 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.1)))
    (tstamp f4cb8144-94d9-4397-bc4e-1ff79ccdc003)
  )
  (fp_text value "KF211V-5.0" (at -5.1 10.8 90 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 502ca16c-5f62-49b6-906e-c769cca7508d)
  )
  (fp_text user "${REFERENCE}" (at -7.7 -10.7 90 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 1ca9ad1b-8e1f-4afb-9fc4-81bc28008fb8)
  )
  (fp_line (start -6.25 -14.75) (end 6.25 -14.75)
    (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp e88726b6-2348-46c7-8eb1-f47699e58dd4))
  (fp_rect (start -6.25 15.75) (end 6.25 -15.75)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.SilkS") (tstamp 579fe4bb-35ec-41df-9487-c5956de12097))
  (pad "1" thru_hole circle (at 0 12.75) (size 2.54 2.54) (drill 1.4) (layers "*.Cu" "*.Mask") (tstamp dc62150b-b6c1-4c38-b459-4c4d9955514d))
  (pad "2" thru_hole circle (at 0 7.75) (size 2.54 2.54) (drill 1.4) (layers "*.Cu" "*.Mask") (tstamp f69fcb26-813f-4b28-b77f-9be5ba5ce27a))
  (pad "3" thru_hole circle (at 0 2.75) (size 2.54 2.54) (drill 1.4) (layers "*.Cu" "*.Mask") (tstamp dfb5a44d-8e5a-45aa-ac3c-ee84963489ae))
  (pad "4" thru_hole circle (at 0 -2.25) (size 2.54 2.54) (drill 1.4) (layers "*.Cu" "*.Mask") (tstamp 4efcbd0e-ccd3-4ec0-bdc7-d059faa64cfb))
  (pad "5" thru_hole circle (at 0 -6.75) (size 2.54 2.54) (drill 1.4) (layers "*.Cu" "*.Mask") (tstamp a86aed4e-357b-45fc-8863-d192556a9c7e))
  (pad "6" thru_hole circle (at 0 -11.75) (size 2.54 2.54) (drill 1.4) (layers "*.Cu" "*.Mask") (tstamp 4745452d-7b46-438c-9c1e-85b61db38ea9))
)
