(footprint "JST_XH_S4B-XH-SM4-TB_1x04-1MP_P2.50mm_Horizontal_Short"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "JST XH series connector, S4B-XH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
	(tags "connector JST XH horizontal")
	(property "Reference" "J1"
		(at 0 -5.5 180)
		(layer "F.SilkS")
		(uuid "5189617f-ae00-4252-85eb-95e3472e388f")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "Signal IN"
		(at 0 6.7 180)
		(layer "F.Fab")
		(uuid "ad9f18c4-ffaf-4531-83f9-08f27c9d0780")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
		(uuid "c91dcd0e-8010-4033-9410-20317d70e288")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "Generic connector, single row, 01x04, script generated"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
		(uuid "393d0786-b1c0-4a31-b602-60194695daac")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -6.81 -1.81)
		(end -4.66 -1.81)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "453d3ba4-e4af-46bf-9ef5-4a910593ef20")
	)
	(fp_line
		(start -6.81 1.34)
		(end -6.81 -1.81)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "7e4af5fb-6037-44d0-b89c-5261ba227577")
	)
	(fp_line
		(start -5.79 5.41)
		(end 5.79 5.41)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "a85bfddb-3776-4eaf-968f-cb315526d067")
	)
	(fp_line
		(start -4.66 -1.81)
		(end -4.66 -4.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "ad4b3f59-d46a-4cc3-959e-583f66df052d")
	)
	(fp_line
		(start 6.81 -1.81)
		(end 4.66 -1.81)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "dab88fc2-d857-42e5-bbad-c98afcd9cadd")
	)
	(fp_line
		(start 6.81 1.34)
		(end 6.81 -1.81)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "09c0139e-4655-40c6-9b46-ff1b90a1ebcd")
	)
	(fp_line
		(start -8.35 -4.5)
		(end -8.35 6)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "63b06c4c-34ab-440a-8dde-5d74623fa047")
	)
	(fp_line
		(start -8.35 6)
		(end 8.35 6)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "c96eb8e1-fca5-4223-9b2f-ef7391095772")
	)
	(fp_line
		(start 8.35 -4.5)
		(end -8.35 -4.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "527b9528-76b4-48b6-87a2-367585a0ecc1")
	)
	(fp_line
		(start 8.35 6)
		(end 8.35 -4.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "b6f6eb93-3a9b-45b7-9be7-e6cabb61d7d7")
	)
	(fp_line
		(start -6.7 -1.7)
		(end -6.7 5.3)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "69e0d91a-312e-48be-b9f4-a23a8fbceb94")
	)
	(fp_line
		(start -6.7 -1.7)
		(end 6.7 -1.7)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "47ca33aa-6195-4a4d-b560-7b7b98659cce")
	)
	(fp_line
		(start -6.7 5.3)
		(end 6.7 5.3)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "786d6ed0-2720-47b1-8745-4db5bd543881")
	)
	(fp_line
		(start -4.25 -1.7)
		(end -3.75 -0.992893)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "ea3e530b-7a3c-41a1-a259-9a321b1f3d36")
	)
	(fp_line
		(start -3.75 -0.992893)
		(end -3.25 -1.7)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "9511fb05-a05e-4a6c-9f98-19dc1acb493f")
	)
	(fp_line
		(start 6.7 -1.7)
		(end 6.7 5.3)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "1feed47e-aa40-4bd9-bd9a-f4119eba483d")
	)
	(fp_text user "${REFERENCE}"
		(at 0 1.5 180)
		(layer "F.Fab")
		(uuid "41f9abe6-b3ac-42cb-9ae6-c2e2ad50de9c")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd roundrect
		(at -3.75 -2.5)
		(size 1.3 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.192308)
		(uuid "d526cf52-f866-438e-a2b5-6217470ee2db")
	)
	(pad "2" smd roundrect
		(at -1.25 -2.5)
		(size 1.3 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.192308)
		(uuid "1e9c2797-b4f0-4c2d-a7b3-ba99119f7a2e")
	)
	(pad "3" smd roundrect
		(at 1.25 -2.5)
		(size 1.3 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.192308)
		(uuid "2725dc47-161c-46f7-9424-a3edc650b579")
	)
	(pad "4" smd roundrect
		(at 3.75 -2.5)
		(size 1.3 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.192308)
		(uuid "97fe7f0f-4ab4-490d-85f5-98c489356a05")
	)
	(pad "MP" smd roundrect
		(at -6.95 3.55)
		(size 1.8 3.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.138889)
		(uuid "39b49afb-f61b-44ce-a4af-ce0f2abaf2a1")
	)
	(pad "MP" smd roundrect
		(at 6.95 3.55)
		(size 1.8 3.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.138889)
		(uuid "7433fe12-34eb-4b10-ba96-f990b4db95cd")
	)
	(embedded_fonts no)
	(model "C:/Users/Frank/Documents/KiCad/9.0/3dmodels/S4B-XH-SM4-TB--3DModel-STEP-56544.STEP"
		(offset
			(xyz 0 -4 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 -0 -0)
		)
	)
)
